IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: f4a0f551-23e2-4268-8098-f470dff90bdc, NumberOfSaves: 8]"
Description: "CoordinateReference [CoordinateBase: Coordenadas compartilhadas, ProjectSite: Terreno padrão]"
File name: "FAMILIAS DE CONCEPT REDUZIDO.ifc"
Time stamp: "2025-03-28T09:42:37"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)"

People and organizations
  Person "JoaoHenriqueSF" of Organization (no name given)
  Owner history of Person "JoaoHenriqueSF" of Organization (no name given) | application "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)" | change NOCHANGE | created 1743083100 (2025-03-27T13:45:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nome do projeto" | phase "Status do projeto"
  IFCSITE "Default" | latitude -15° 52′ 0.12062″ | longitude -47° 55′ 0.11444″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Insira aqui o endereço", "Brasília", "Brasil"
      IFCBUILDINGSTOREY "Nível 1" | long name "Nível 1" | object type "Nível:Cabeça de 8 mm" | elevation 0.
        contains 41 elements
          1 x IFCROOF | type IFCCURTAINWALLTYPE "Vidraça inclinada:PV_Benchmark-Concept-MX01.0_NS_038mm" | object type "Vidraça inclinada:PV_Benchmark-Concept-MX01.0_NS_038mm" | names: "Vidraça inclinada:PV_Benchmark-Concept-MX01.0_NS_038mm:291576" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PS 11.0-R:PS 11.0-R" | object type "PS 11.0-R:PS 11.0-R" | names: "PS 11.0-R:PS 11.0-R:329096", "PS 11.0-R:PS 11.0-R:349335", "PS 11.0-R:PS 11.0-R:361239" | material: "RAL5010" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 13.0-R:MX 13.0-R" | object type "MX 13.0-R:MX 13.0-R" | names: "MX 13.0-R:MX 13.0-R:329100", "MX 13.0-R:MX 13.0-R:353727", "MX 13.0-R:MX 13.0-R:361237" | material: "RAL5010" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 14.0-R:MX 14.0-R" | object type "MX 14.0-R:MX 14.0-R" | names: "MX 14.0-R:MX 14.0-R:329102", "MX 14.0-R:MX 14.0-R:329644", "MX 14.0-R:MX 14.0-R:361236" | material: "RAL6003" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 15.0-R:MX 15.0-R" | object type "MX 15.0-R:MX 15.0-R" | names: "MX 15.0-R:MX 15.0-R:329104", "MX 15.0-R:MX 15.0-R:329643", "MX 15.0-R:MX 15.0-R:361235" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 16.0-R:MX 16.0-R" | object type "MX 16.0-R:MX 16.0-R" | names: "MX 16.0-R:MX 16.0-R:329106", "MX 16.0-R:MX 16.0-R:349391", "MX 16.0-R:MX 16.0-R:361234" | material: "RAL1015" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PS 10.0-R:PS 10.0-R" | object type "PS 10.0-R:PS 10.0-R" | names: "PS 10.0-R:PS 10.0-R:329108", "PS 10.0-R:PS 10.0-R:349392", "PS 10.0-R:PS 10.0-R:361233" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCROOF | type IFCCURTAINWALLTYPE "Vidraça inclinada:PH_Benchmark-Concept-MX01.0_NS_038mm" | object type "Vidraça inclinada:PH_Benchmark-Concept-MX01.0_NS_038mm" | names: "Vidraça inclinada:PH_Benchmark-Concept-MX01.0_NS_038mm:329599" | property sets: Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Pset_RoofCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 12.0-R:MX 12.0-R" | object type "MX 12.0-R:MX 12.0-R" | names: "MX 12.0-R:MX 12.0-R:329646", "MX 12.0-R:MX 12.0-R:361063", "MX 12.0-R:MX 12.0-R:361238" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Parede cortina:PH_Benchmark-Concept-MX01.0_EW_038mm" | object type "Parede cortina:PH_Benchmark-Concept-MX01.0_EW_038mm" | names: "Parede cortina:PH_Benchmark-Concept-MX01.0_EW_038mm:360270" | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 12.0-R:MX 12.0-R" | object type "MX 12.0-R:MX 12.0-R" | names: "MX 12.0-R:MX 12.0-R:360292", "MX 12.0-R:MX 12.0-R:360299" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 13.0-R:MX 13.0-R" | object type "MX 13.0-R:MX 13.0-R" | names: "MX 13.0-R:MX 13.0-R:360293", "MX 13.0-R:MX 13.0-R:360300" | material: "RAL5010" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 14.0-R:MX 14.0-R" | object type "MX 14.0-R:MX 14.0-R" | names: "MX 14.0-R:MX 14.0-R:360294", "MX 14.0-R:MX 14.0-R:360301" | material: "RAL6003" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 15.0-R:MX 15.0-R" | object type "MX 15.0-R:MX 15.0-R" | names: "MX 15.0-R:MX 15.0-R:360295", "MX 15.0-R:MX 15.0-R:360302" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "MX 16.0-R:MX 16.0-R" | object type "MX 16.0-R:MX 16.0-R" | names: "MX 16.0-R:MX 16.0-R:360296", "MX 16.0-R:MX 16.0-R:360303" | material: "RAL1015" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PS 10.0-R:PS 10.0-R" | object type "PS 10.0-R:PS 10.0-R" | names: "PS 10.0-R:PS 10.0-R:360297", "PS 10.0-R:PS 10.0-R:360304" | material: "RAL3000" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PS 11.0-R:PS 11.0-R" | object type "PS 11.0-R:PS 11.0-R" | names: "PS 11.0-R:PS 11.0-R:360298", "PS 11.0-R:PS 11.0-R:360305" | material: "RAL5010" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Parede cortina:PV_Benchmark-Concept-MX01.0_NS_038mm" | object type "Parede cortina:PV_Benchmark-Concept-MX01.0_NS_038mm" | names: "Parede cortina:PV_Benchmark-Concept-MX01.0_NS_038mm:361219" | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Piso:Concreto-comercial 200 mm" | object type "Piso:Concreto-comercial 200 mm" | FLOOR | names: "Piso:Concreto-comercial 200 mm:361373" | material: layers "Piso:Concreto-comercial 200 mm" ("Concreto, Moldado in loco" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | object type "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | names: "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range:361387" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Nível 2" | long name "Nível 2" | object type "Nível:Cabeça de 8 mm" | elevation 3999.9999999999995

Types
  IFCCURTAINWALLTYPE "Vidraça inclinada:PV_Benchmark-Concept-MX01.0_NS_038mm" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PS 11.0-R:PS 11.0-R" | 3 occurrences | material: "RAL5010" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 13.0-R:MX 13.0-R" | 3 occurrences | material: "RAL5010" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 14.0-R:MX 14.0-R" | 3 occurrences | material: "RAL6003" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 15.0-R:MX 15.0-R" | 3 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 16.0-R:MX 16.0-R" | 3 occurrences | material: "RAL1015" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PS 10.0-R:PS 10.0-R" | 3 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Vidraça inclinada:PH_Benchmark-Concept-MX01.0_NS_038mm" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 12.0-R:MX 12.0-R" | 3 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Parede cortina:PH_Benchmark-Concept-MX01.0_EW_038mm" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 12.0-R:MX 12.0-R" | 2 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 13.0-R:MX 13.0-R" | 2 occurrences | material: "RAL5010" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 14.0-R:MX 14.0-R" | 2 occurrences | material: "RAL6003" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 15.0-R:MX 15.0-R" | 2 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "MX 16.0-R:MX 16.0-R" | 2 occurrences | material: "RAL1015" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PS 10.0-R:PS 10.0-R" | 2 occurrences | material: "RAL3000" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PS 11.0-R:PS 11.0-R" | 2 occurrences | material: "RAL5010" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Parede cortina:PV_Benchmark-Concept-MX01.0_NS_038mm" | 1 occurrence | property sets: Pset_CurtainWallCommon, Pset_ManufacturerTypeInformation
  IFCSLABTYPE "Piso:Concreto-comercial 200 mm" | FLOOR | 1 occurrence | material: layers "Piso:Concreto-comercial 200 mm" ("Concreto, Moldado in loco" 200.) | property sets: Pset_SlabCommon
  IFCBUILDINGELEMENTPROXYTYPE "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | 1 occurrence | material: "<Unnamed>"

Property sets
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCROOF) | on 16 type objects
    Manufacturer = "Kingspan Isoeste" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 2 type objects
    Manufacturer = "victor.monteiro@kingspanisoeste.com.br" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "PS 11.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 13.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 14.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 15.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 16.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "PS 10.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 12.0-R" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCROOF)
    Reference = "PV_Benchmark-Concept-MX01.0_NS_038mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 4 more contents on 4 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 1.9600000004267162 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PV_Benchmark-Concept-MX01.0_NS_038mm" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 1.9600000000000004 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PH_Benchmark-Concept-MX01.0_NS_038mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "PS 11.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 13.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 14.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 15.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 16.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "PS 10.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY)
    Reference = "MX 12.0-R" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Kingspan Isoeste Color Range" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "PH_Benchmark-Concept-MX01.0_EW_038mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "PV_Benchmark-Concept-MX01.0_NS_038mm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Concreto-comercial 200 mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concreto-comercial 200 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 5.2300000000000004 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)