IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "RevitIdentifiers [VersionGUID: 061e6111-021b-426b-ac3a-857ebf0343b1, NumberOfSaves: 18]"
Description: "CoordinateReference [CoordinateBase: Coordenadas compartilhadas]"
File name: "1 - Família Lumini.ifc"
Time stamp: "2025-04-04T09:43:03"
Preprocessor: "ODA IFC SDK 22.8"
Originating system: "22.1.80.32 - IFC 22.7.0.0 - Default UI"
Application: "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)"

People and organizations
  Person "JoaoHenriqueSF" of Organization (no name given)
  Owner history of Person "JoaoHenriqueSF" of Organization (no name given) | application "Autodesk Revit 2022 (PTB)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (PTB)" | change NOCHANGE | created 1743510083 (2025-04-01T12:21:23Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  IONCONCENTRATIONUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  THERMALCONDUCTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  MASSFLOWRATEUNIT: derived
  ROTATIONALFREQUENCYUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  ENERGYUNIT: JOULE
  USERDEFINED: derived "Luminous Efficacy"
  USERDEFINED: derived "Electrical Resistivity"
  SOUNDPOWERUNIT: derived
  SOUNDPRESSUREUNIT: derived
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived
  SPECIFICHEATCAPACITYUNIT: derived
  HEATFLUXDENSITYUNIT: derived
  HEATINGVALUEUNIT: derived
  VAPORPERMEABILITYUNIT: derived
  DYNAMICVISCOSITYUNIT: derived
  THERMALEXPANSIONCOEFFICIENTUNIT: derived
  MODULUSOFELASTICITYUNIT: derived
  ISOTHERMALMOISTURECAPACITYUNIT: derived
  MOISTUREDIFFUSIVITYUNIT: derived
  MASSPERLENGTHUNIT: derived
  THERMALRESISTANCEUNIT: derived
  ACCELERATIONUNIT: derived
  ANGULARVELOCITYUNIT: derived
  LINEARSTIFFNESSUNIT: derived
  WARPINGCONSTANTUNIT: derived
  LINEARMOMENTUNIT: derived
  TORQUEUNIT: derived

Spatial structure
IFCPROJECT "0001" | long name "Nome do projeto" | phase "Status do projeto"
  IFCSITE "Default" | latitude -15° 52′ 0.12062″ | longitude -47° 55′ 0.11444″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Insira aqui o endereço", "Brasília", "Brasil"
      IFCBUILDINGSTOREY "Nível 1" | long name "Nível 1" | object type "Nível:Cabeça de 8 mm" | elevation 0.
        contains 30 elements
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Parede cortina:PH_PAINEL LYNEAR 50MM" | object type "Parede cortina:PH_PAINEL LYNEAR 50MM" | names: "Parede cortina:PH_PAINEL LYNEAR 50MM:291643" | parts: 9 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          1 x IFCSLAB | type IFCSLABTYPE "Piso:Concreto-comercial 200 mm" | object type "Piso:Concreto-comercial 200 mm" | FLOOR | names: "Piso:Concreto-comercial 200 mm:315778" | material: layers "Piso:Concreto-comercial 200 mm" ("Concreto, Moldado in loco" 200.) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Parede cortina:PV_PAINEL LYNEAR 50MM" | object type "Parede cortina:PV_PAINEL LYNEAR 50MM" | names: "Parede cortina:PV_PAINEL LYNEAR 50MM:316121" | parts: 12 IFCMEMBER | property sets: Pset_CurtainWallCommon, Pset_QuantityTakeOff
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:350338", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:350348", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:355681" (+3 more) | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:350354", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:350355" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388460", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388462" | material: "Policarbonato" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388463" | material: "Policarbonato" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388468", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388469" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:388470" | material: "Policarbonato" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCROOF | type IFCCURTAINWALLTYPE "Vidraça inclinada:PV_PAINEL LYNEAR 50MM" | object type "Vidraça inclinada:PV_PAINEL LYNEAR 50MM" | names: "Vidraça inclinada:PV_PAINEL LYNEAR 50MM:534245", "Vidraça inclinada:PV_PAINEL LYNEAR 50MM:563202" | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:537530" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:555599", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:563243" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          2 x IFCROOF | type IFCCURTAINWALLTYPE "Vidraça inclinada:PH_PAINEL LYNEAR 50MM" | object type "Vidraça inclinada:PH_PAINEL LYNEAR 50MM" | names: "Vidraça inclinada:PH_PAINEL LYNEAR 50MM:555639", "Vidraça inclinada:PH_PAINEL LYNEAR 50MM:563235" | property sets: Pset_QuantityTakeOff, Pset_RoofCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:556683", "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:563213" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:556685" | material: "Policarbonato" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:563210" | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | object type "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | names: "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM:563244" | material: "Policarbonato" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | object type "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | names: "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range:567946" | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "Nível 2" | long name "Nível 2" | object type "Nível:Cabeça de 8 mm" | elevation 3999.9999999999995

Types
  IFCCURTAINWALLTYPE "Parede cortina:PH_PAINEL LYNEAR 50MM" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCSLABTYPE "Piso:Concreto-comercial 200 mm" | FLOOR | 1 occurrence | material: layers "Piso:Concreto-comercial 200 mm" ("Concreto, Moldado in loco" 200.) | property sets: Pset_SlabCommon
  IFCCURTAINWALLTYPE "Parede cortina:PV_PAINEL LYNEAR 50MM" | 1 occurrence | property sets: Pset_CurtainWallCommon
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 6 occurrences | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 2 occurrences | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 2 occurrences | material: "Policarbonato" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "Policarbonato" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 2 occurrences | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "Policarbonato" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Vidraça inclinada:PV_PAINEL LYNEAR 50MM" | 2 occurrences | property sets: Pset_CurtainWallCommon
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 2 occurrences | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCCURTAINWALLTYPE "Vidraça inclinada:PH_PAINEL LYNEAR 50MM" | 2 occurrences | property sets: Pset_CurtainWallCommon
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 2 occurrences | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "Policarbonato" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "POLICARBONATO BRANCO OPACO" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "PAINEL LUMINI 38MM:PAINEL LUMINI 38MM" | 1 occurrence | material: "Policarbonato" | property sets: Pset_ManufacturerTypeInformation
  IFCBUILDINGELEMENTPROXYTYPE "32-KS-ISO-Colour Range:Kingspan Isoeste Color Range" | 1 occurrence | material: "<Unnamed>"

Property sets
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "PH_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "PV_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 type objects
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_QuantityTakeOff | properties | on 22 objects (22 IFCBUILDINGELEMENTPROXY)
    Reference = "PAINEL LUMINI 38MM" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCMEMBER)
    Reference = "Estrutura Auxiliar ao Lynear - Emenda" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCMEMBER)
    Reference = "Estrutura Auxiliar ao Lynear - Final Esquerdo" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 7 objects (7 IFCMEMBER)
    Reference = "Estrutura Auxiliar ao Lynear - Final Direito" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (2 IFCROOF, 1 IFCCURTAINWALL)
    Reference = "PH_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 3 objects (2 IFCROOF, 1 IFCCURTAINWALL)
    Reference = "PV_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCSLAB)
    Reference = "Concreto-comercial 200 mm" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Kingspan Isoeste Color Range" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Emenda" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Final Esquerdo" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Final Esquerdo" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Emenda" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 2 objects (2 IFCMEMBER)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Final Direito" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Emenda" (IFCIDENTIFIER)
    Span = 500.00000000000006 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Final Esquerdo" (IFCIDENTIFIER)
    Span = 500.00000000000006 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "Estrutura Auxiliar ao Lynear - Final Direito" (IFCIDENTIFIER)
    Span = 1000.0000000000001 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_MemberCommon: 8 more contents on 8 objects not shown
  Pset_ReinforcementBarPitchOfSlab | properties | on 1 object (1 IFCSLAB)
    Reference = "Concreto-comercial 200 mm" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "Concreto-comercial 200 mm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 5.2300000000000004 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_BuildingElementProxyCommon | properties | on 22 objects (22 IFCBUILDINGELEMENTPROXY)
    Reference = "PAINEL LUMINI 38MM" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Kingspan Isoeste Color Range" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2.2500000000000098 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PV_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2.2500000000000067 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PH_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2.2500000000000075 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PV_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 2.2500000000000053 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "PH_PAINEL LYNEAR 50MM" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 2 objects (2 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Pset_ManufacturerTypeInformation | properties | on 12 type objects
    Manufacturer = "Kingspan Isoeste" (IFCLABEL)